Trimble Navigation Ltd.	Engineering Document		2/18/94 EFJ

Serial EEPROM configuration load program - Program SEELDxxx.EXE

(xxx is replaced by a version number, i.e. SEELD001.EXE)

This program has a specific SEEPROM configuration compiled into its 
executable. The program requires that a Trimble GPS sensor is connected via a 
serial port (COM1 or COM2) to a IBM compatible PC. When SEELDxxx is run, 
its internal configuration is written to the SEEPROM. 

Caution!! The SEEPROM configuration previously stored in the sensor is 
destroyed.

The SEELDxxx prompts the user:

	1) Connect the GPS sensor to COMx.	(x= 1 or 2)
	2) Power off, then on the GPS sensor.

	Then SEELDxxx establishes communications with the GPS sensor.
	Loads it’s internal configuration to the SEEPROM.

	3) Informs user of success or failure.
	4) Do you wish to load another GPS SEEPROM? [y=yes, n=no]
	5) If "y": Power off and disconnect the GPS sensor.   (goto #1 above)
	6) If "n": Program is now complete.

If the user chooses to do so, SEELDxxx will run again, and again.. until the 
user answers "n" (n=no).

For HELP on program operation, run the program with any of the following 
command line parameters; {?, h, H}, i.e. 	SEELD001 ?
